
================================================================================
Winsock Performance Test Procedures:
	1. Run "perf_winsockd2 -debug" command under a Windows Desktop (IP=192.168.0.1) 
	    to startup Winsock Performance Test Server.
	2. Start Windows CE Test Kit (CETK) on the Platform Builder machine.
	3. Select "Start client..." from the "Connection" menu.
	4. On the "Device Connection" dialog, make sure the "Use Windows Sockets
	   for the client/server communication." checkbox is NOT checked.
	5. Click "Connect..." to get the connection to Windows CE target device.
	6. On the "Select a Windows CE Device" dialog, select the device you are
	   connecting to (typically "Default Device") and click OK.
	7. Select "Windows CE Device Driver Test Kit" and click right mouse key 
	   to select "Deselect All Tests".
	8. Expand the "Ethernet" test items under "Windows CE Device Driver Test Kit".
	9. Select "Performance Tests" --> "Winsock Performance Test" and click right mouse key 
	   to select "Edit Command Line...". Enter 
	   <tux -o -d perf_winsock2 -x 1001 -x 1002 -c "-s 192.168.0.1 -i 4">
	   command on the Edit Command Line dialog and click OK.
	10.Select "Windows CE Device Driver Test Kit" and click right mouse key 
	   to select "Start Tests" to start the Ethernet testings.
================================================================================



